### Tinkerforge Brick Daemon installation

Install the TinkerForge Brick Daemon on a Raspberry Pi with hardware floating point unit support (Raspbian).
References
Raspberry Pi
http://www.tinkerforge.com/en/doc/Embedded/Raspberry_Pi.html
Brick Daemon
http://www.tinkerforge.com/en/doc/Software/Brickd.html
Steps
Login as Pi
Installation
$sudo apt-get install libusb-1.0-0 libudev0 pm-utils
$wget http://download.tinkerforge.com/tools/brickd/linux/brickd_linux_latest_armhf.deb
$sudo dpkg -i brickd_linux_latest_armhf.deb
The Brick Daemon will be started after the installation and at startup automatically.
Updates
$wget http://download.tinkerforge.com/tools/brickd/linux/brickd_linux_latest_armhf.deb
$sudo dpkg -i brickd_linux_latest_armhf.deb
Logging
Windows
Reported in the Windows Event Log.
Use the logviewer.exe tool (part of brickd installation) to view the Windows Event Log filtered for brickd messages.
Linux and Mac OS X
Log messages are written to /var/log/brickd.log.
Configuration
Windows:
C:\Program Files\Tinkerforge\Brickd\brickd.ini
Linux and Mac OS X:
/etc/brickd.conf
Restart
Windows:
Open "Computer Management", navigate to the "Services" section and restart the Brick Daemon service.
Linux:
sudo /etc/init.d/brickd restart
Mac OS X:
sudo launchctl stop com.tinkerforge.brickd
sudo launchctl start com.tinkerforge.brickd

Changed: , Category: Domoticz Home Automation, File: T6C186M1357.htm, ID: 1357