### MQTT

To be able to use Domoticz MQTT as described here http://www.domoticz.com/wiki/MQTT an MQTT Hardware Device has to be defined in Domoticz.
This is important! means do not forget (saw several forum discussions about this).
Setup > Hardware:
Type: MQTT Client Gateway with LAN Interface
Remote Address: 192.168.0.29 (THIS AS AN EXAMPLE IP)
Port: 1883 (The default MQTT port)
Name: MQTT Client
Then save and check the Domoticz log, if the MQTT service has started and if messages arrive using topic "domoticz/in".

Changed: , Category: Domoticz Home Automation, File: T6C186M1351.htm, ID: 1351