### Set Static IP Address

To set a Static IP address, two options, but Option 1 preferred.
Option 1
Set static IP address via the Brick Viewer:
Select settings and configure the Network with a fixed IP Address:
WPA Key: yourkey
Address: Static
IP: 192.168.0.30
Subnet mask: 255.255.255.0
Gateway: 192.168.0.1
DNS: 192.168.0.1
Option 2
Login as user tf.
Obtain Gateway Address
$netstat -r -n
Set root priviledges
$sudo -s
Set Static IP Address
Edit:
$sudo nano /etc/network/interfaces
Replace
iface eth0 inet dhcp
By (with example data)
iface eth0 inet static
address 192.168.178.28
netmask 255.255.255.0
gateway 192.168.178.1
Then reboot.

Changed: , Category: TinkerForge RED Brick, File: T6C268M2000.htm, ID: 2000