### Install Brick Daemon on Raspberry Pi

Install the TinkerForge Brick Daemon on a Raspberry Pi with hardware floating point unit support (Raspbian).
Reference: http://www.tinkerforge.com/en/doc/Embedded/Raspberry_Pi.html
Login as Pi
Install
sudo apt-get install libusb-1.0-0 libudev0 pm-utils
wget http://download.tinkerforge.com/tools/brickd/linux/brickd_linux_latest_armhf.deb
sudo dpkg -i brickd_linux_latest_armhf.deb
The Brick Daemon will be started after the installation and at startup automatically.
The configuration file is located in /etc/brickd.conf and be edited as sudo nano /etc/brickd.conf.
Updates
wget http://download.tinkerforge.com/tools/brickd/linux/brickd_linux_latest_armhf.deb
sudo dpkg -i brickd_linux_latest_armhf.deb

Changed: 2017-12-05 13:32, Category: TinkerForge, File: T6C264M1963.htm, ID: 1963