### B4J MQTT Setup

B4X jMQTT CLIENT LIBRARY
Reference jMQTT Official MQTT client:
http://www.b4x.com/android/forum/threads/iot-mqtt-protocol.59471/
Installation Steps (based Raspian Jessie)
sudo wget http://repo.mosquitto.org/debian/mosquitto-jessie.list
sudo apt-get update
sudo apt-get install mosquitto mosquitto-clients
Check if Mosquitto running
ps -A | grep mosq
Output example:
5723 ? 00:00:00 mosquitto
Mosquitto starts automatically after every boot
Startup script located in: /etc/init.d/mosquitto
Mosquitto Control
sudo service mosquitto restart
sudo service mosquitto stop
sudo service mosquitto start
Examples
• See B4J HowTo Category MQTT

Changed: 2018-06-07 09:19, Category: Raspberry Pi MQTT, File: T6C236M1726.htm, ID: 1726